# İKİLİ FİLTRE DIŞ KABI



APPLICATIONS

Filtration and treatment of water with neutral pH and drinking water. The exclusive Duplex housings allow faster and safer installation of serial filtration units.



**Medium**

**Junior**

**Master**

**Senior**

**Domestic use:** filtration and treatment of drinking water, protection of taps, boilers, washing machines, and other installations.

**Technical use:** pre-filtration, micro-filtration; protection of pumps, heating systems, softeners, demineralising and chlorine-removing appliances, reverse osmosis units.

WORKING CONDITIONS

Max working pressure 8 BAR Max working temperature 45°C

SPECIFICATIONS

Non-toxic materials, suitable for drinking water. **Head and ring nut:** reinforced polypropylene. **Transparent bowl:** SAN.

**O-ring:** ETP.

**Breather-valve:** body polypropylene, O-ring ETP.

**IN/OUT threads:** CW 614 N brass inserts.



**B**

**A**

**VARIANTS** available on minimum quantity

**FP** female plastic IN/OUT **AB** housings with opaque threads, BSP type 3/4”. bowl, impermeable to the

light.

**accessories**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Cartridge height** | **housings with transparent bowl AS IN/OUT female threads with FO brass inserts** | **IN/OUT**  **threads** | **mm** | |
| **A** | **B** |
| 10” | Senior Duplex Plus 3P AFO SX AS | 3/4” | 315 | 275 |
|  |  |  |  |  |

